Y2 Dongyi Law Enforcement Recorder
Product Specification (Model: Y2东一执法记录仪)
Product Information
	Appearance Name
	Y Series

	Series Model
	Y2东一执法记录仪


Six Views
	[image: ]


Function Diagram
	[image: ]


Basic Information
	processor
	no

	operating system
	no

	Screen size
	2.0 inch horizontal screen

	Default battery capacity
	3500mAh

	Optional battery capacity upgrade
	no

	charging duration
	3 hours

	Continuous recording duration
	Approximately 15 hours Approximately 16 hours

	standby time
	about 18 hours

	anti-shake
	no

	image format
	MP4

	compression format
	H.264/H.265

	Video size
	Maximum 2K(2560*1440)30FPS

	photo format
	JPEG

	horn
	1.5W

	body memory
	Scalable up to 512G

	Rear camera (main)
	200W

	Photo size
	Maximum 80 million


Lighting
	laser lamp
	Support auxiliary locking imaging center or laser marking

	white light Lamp
	have

	alarm lamp
	Red and blue warning lights

	infrared lamp
	have


Interfaces
	charging interface
	Type-C

	G-sensor
	support

	vibration motor
	not support

	external camera
	support

	charging method
	Complete line charging

	charger
	5V-1A

	USB interface
	USB 2.0


Data Functions
	WIFI
	Point-to-point AP-wifi is optional

	Bluetooth/433
	no

	positioning
	no


Dimensions
	Length (mm)
	56

	Height (mm)
	89

	Thickness (mm)
	27

	Weight (g) Approx
	170


Basic Device Functions
	Video pre-recording
	--------------------

	Video extension
	--------------------

	Impact alarm
	--------------------

	night vision
	Automatic or manual night vision switching, support for high-power red lights

	fill light
	--------------------

	USB flash drive function
	Drive mode: After connecting to the computer, you can enter the USB flash drive mode (removable hard disk) through the upper computer on the PC side;
Non-drive mode: After connecting to the computer, directly enter USB flash drive mode (removable hard disk); one of the two modes can be selected

	menu language
	Default Simplified Chinese/English (other languages can be customized)

	Key Document Marker
	You can mark this video file by pressing the corresponding button during the recording process;

	continuous shooting function
	The supporting device can take more than 10 photos continuously at one time

	password protection function
	support

	Close beat mode
	Support no indicator light display and no sound reminder mode.

	Shooting in the middle
	During the recording process, press the shoot button to take a photo individually

	video encryption
	--------------------

	automatically overwritten
	Support automatic override/non-override

	in-vehicle functions
	Support vehicle-mounted certificate collection, and realize automatic video recording and evidence collection when the car ignites and turns on, and automatic shutdown after parking and flameout.

	safe mode
	Safe mode is limited to basic operations such as recording, taking photos, and recording. A password is required to enter the settings interface and playback interface.

	acquisition station
	Support collection station and background management 1. Operation logs;2. Data collection and classification

	data security management
	Law enforcement recorders have different authority management. Primary authority can only view and playback law enforcement videos, photos, and recordings, and cannot delete or modify sensitive settings of the machine. Sensitive settings of the machine can only be made through password verification, and can only be copied, modified or deleted after connecting to a computer.

	motion detection
	--------------------

	One-click shortcut function
	--------------------


Others
	protection grade
	--------------------

	injection molding process
	--------------------

	low-temperature compatibility
	Corresponding low-temperature batteries should be prepared for inspection and low-temperature areas. The low-temperature-30 ℃ battery life of a single battery should be more than 2 hours. Normal temperature batteries should be standard. Normal temperature batteries and low-temperature batteries have different densities and operating environments.

	Storage relative humidity
	63%(30℃)

	storage temperature
	-40~60℃

	operating relative humidity
	40%~80%

	operating temperature
	-20~55℃


Packing Information
	Box gauge: length × width × height mm
	

	Weight of the whole box:
	

	Number of boxes:
	--------------------

	Package: L × W × H mm
	

	Net weight of packaging box:
	

	Machine net weight:
	

	Weight of outer packaging box:
	550g


Standard Accessories
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Universal Optional Accessories
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Polyester shoulder strap
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Polyester single shoulder strap
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Reflective shoulder straps
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Reflective shoulder strap
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Shoulder straps on both shoulders
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BABBH Single shoulder strap
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Wear law enforcement device accessories
leather case on the chest
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Law enforcement equipment accessorieslather cover
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Anti slip fixed headband bracket
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B1TZEX 2 bicycle stand
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A FF Walkie talkie clip
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28R Crocodile back clip
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Car suction cup holder
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360 degree metal head long shoulder clip
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180 degree plastic head long shoulder clip
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