AWS-CAT1-4G Law Enforcement Recorder-Built-in Battery-851
Product Specification (Model: AWS-CAT1-4G执法记录仪-内置电池-851)
Product Information
	Appearance Name
	AWS-CAT1-4G Law Enforcement Recorder-Built-in Battery-851

	Series Model
	AWS-CAT1-4G执法记录仪-内置电池-851


Six Views
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Function Diagram
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Basic Information
	processor
	Quan Zhi 851

	operating system
	Linux

	Screen size
	--------------------

	Default battery capacity
	3000mAh

	Optional battery capacity upgrade
	4200mAh

	charging duration
	3 hours

	Continuous recording duration
	about 13 hours

	standby time
	empty

	anti-shake
	no

	image format
	MP4

	compression format
	H.264/H.265

	Video size
	Maximum 2K(2560*1440)30FPS

	photo format
	JPEG

	horn
	1W

	body memory
	Scalable up to 512G

	Rear camera (auxiliary AF)
	no

	Front camera (screen)
	no

	Rear camera (main)
	200W(optional 400W)

	Photo size
	Maximum 54 million

	noise reduction module
	not support


Lighting
	laser lamp
	Support auxiliary locking imaging center or laser marking

	alarm lamp
	Red and blue warning lights

	infrared lamp
	have

	white light Lamp
	have


Interfaces
	charging interface
	Type-C

	headphone jack
	no

	G-sensor
	support

	vibration motor
	not support

	external camera
	support

	charging base
	not support

	charging method
	Complete line charging

	charger
	5V-2A

	USB interface
	USB 2.0


Data Functions
	Sim/TF Card Slot
	Single Sim Single TF

	WIFI
	WIFI5.8 a/b/g/n/ac

	Bluetooth/433
	no

	positioning
	(Optional Beidou) Multi-mode Global GLONASS+GPS+Galileo+Compass

	compass
	not support

	air pressure sensor
	not support

	temperature sensor
	not support

	ambient light sensor
	not support

	NFC
	no

	encryption card
	not support


Dimensions
	Length (mm)
	55.2

	Height (mm)
	87.3

	Thickness (mm)
	40

	Weight (g) Approx
	145


Other Network Functions
	video intercom
	Support law enforcement instrument to platform single and two-way video intercom, support law enforcement instrument end-to-end single and two-way video intercom (requires integration of third-party software SDK)

	Voice cluster intercom
	Support group intercom, end-to-end intercom

	voice broadcast
	Support TTS voice broadcast

	voice control
	not support

	Facial and license plate recognition
	not support

	network standard
	Eurasian frequency band
LTE-FDD: B1/B3/B5/B8 LTE-TDD: B34/B38/B39/B40/B41 Other frequency bands are optional

	Platform Administration software
	Support real-time preview/real-time positioning/trajectory playback/intercom/monitoring/remote command issuance, etc.(support secondary development of API calls, independent platform deployment, or secondary independent development of independent key values)

	text overlay
	Support stacking time, equipment number, law enforcement officer number, location information, speed information, and support stacking in Chinese

	Command and dispatch platform docking
	Support protocols: Support platforms such as 808, GB/T28181, RTMP, RTSP, ONVIF protocols and other mainstream protocols in the market to connect with audio and video, intercom, and location device information.


Basic Device Functions
	Video extension
	support

	Video pre-recording
	support

	Impact alarm
	Support airbag security. The product needs to have a G sensor, which can record drops and record collisions. If it has a 4G function, it can be linked in the background.

	video encryption
	not support

	night vision
	Automatic or manual night vision switching, support for high-power red lights

	fill light
	Support the use of white LEDs for auxiliary lighting in dark situations.

	menu language
	Default Simplified Chinese/English (other languages can be customized)

	USB flash drive function
	Drive mode: After connecting to the computer, you can enter the USB flash drive mode (removable hard disk) through the upper computer on the PC side;
Non-drive mode: After connecting to the computer, directly enter USB flash drive mode (removable hard disk); one of the two modes can be selected

	continuous shooting function
	The supporting device can take more than 10 photos continuously at one time

	Key Document Marker
	You can mark this video file by pressing the corresponding button during the recording process;

	One-click shortcut function
	Support one-click quick start of recording, one-click start of recording function (no need to start the power button separately)

	password protection function
	support

	in-vehicle functions
	Support vehicle-mounted certificate collection, and realize automatic video recording and evidence collection when the car ignites and turns on, and automatic shutdown after parking and flameout.

	Shooting in the middle
	During the recording process, press the shoot button to take a photo individually

	acquisition station
	Support collection station and background management 1. Operation logs;2. Data collection and classification

	data security management
	Law enforcement recorders have different authority management. Primary authority can only view and playback law enforcement videos, photos, and recordings, and cannot delete or modify sensitive settings of the machine. Sensitive settings of the machine can only be made through password verification, and can only be copied, modified or deleted after connecting to a computer.

	automatically overwritten
	Support automatic override/non-override

	Close beat mode
	Support no indicator light display and no sound reminder mode.

	safe mode
	Safe mode is limited to basic operations such as recording, taking photos, and recording. A password is required to enter the settings interface and playback interface.


Others
	protection grade
	IP68 fell 2 meters

	injection molding process
	Two-color mold process (anti-crack)

	operating temperature
	-20~55℃

	low-temperature compatibility
	Corresponding low-temperature batteries should be prepared for inspection and low-temperature areas. The low-temperature-30 ℃ battery life of a single battery should be more than 2 hours. Normal temperature batteries should be standard. Normal temperature batteries and low-temperature batteries have different densities and operating environments.

	Storage relative humidity
	63%(30℃)

	storage temperature
	-40~60℃

	operating relative humidity
	40%~80%


Standard Accessories
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Universal Optional Accessories
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Polyester shoulder strap
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Polyester single shoulder strap
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Reflective shoulder straps
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Reflective shoulder strap
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Shoulder straps on both shoulders
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BABBH Single shoulder strap
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Wear law enforcement device accessories
leather case on the chest
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Law enforcement equipment accessorieslather cover
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Anti slip fixed headband bracket
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B1TZEX 2 bicycle stand
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TR MIFE Magnetic chest clip
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B3 Shoulder clip




image22.jpg
B#T3% Shoulder lamp clip
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A FF Walkie talkie clip
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28R Crocodile back clip
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Car suction cup holder
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fase Chest clip
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360 degree metal head long shoulder clip
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180 degree plastic head long shoulder clip
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4@B¥K Shortshoulder clip
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B% Shoulder clip (2)
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Waterproof leather case
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