C6- 4G-Android Spec
Product Specification (Model: C6)
Product Information
	Appearance Name
	

	Series Model
	C6

	Features
	The industry's smallest Android 4G-large system-CAT4 audio and video recorder, domestic low-power chip
IP68 two-color mold, 500W real main camera
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	[image: ]


Basic Information
	processor
	Zhanrui SL8541E quad-core 1.4GHz

	operating system
	Android 12

	Screen size
	2.4 Inch multi-touch screen

	Default battery capacity
	3000mAh

	Optional battery capacity upgrade
	no

	charging duration
	3 hours

	Continuous recording duration
	about 8.5 hours

	standby time
	>300 hours without APP, depending on APP

	anti-shake
	no

	image format
	MP4

	compression format
	H264

	Video size
	Max. 1080P (1920*1080)30FPS

	photo format
	JPEG

	horn
	1.5W

	body memory
	Standard 1+8G, expandable up to 512G

	Rear camera (auxiliary AF)
	no

	Front camera (screen)
	no

	Rear camera (main)
	500W

	Photo size
	Maximum 48 million

	noise reduction module
	not support


Lighting
	laser lamp
	no

	alarm lamp
	Red and blue warning lights

	infrared lamp
	have

	white light Lamp
	have


Interfaces
	charging interface
	Type-C

	headphone jack
	Type-C

	G-sensor
	support

	vibration motor
	support

	external camera
	support

	charging base
	not support

	charging method
	Complete line charging

	charger
	5V-2A

	USB interface
	USB 2.0


Data Functions
	Sim/TF Card Slot
	Single Sim Single TF

	WIFI
	WIFI5.8 a/b/g/n/ac

	Bluetooth/433
	BT5.0(BR/EDR + BLE) supports Bluetooth remote control, Bluetooth voice, Bluetooth tag positioning, etc.

	positioning
	(Optional Beidou) Multi-mode Global GLONASS+GPS+Galileo+Compass

	compass
	support

	air pressure sensor
	support

	temperature sensor
	support

	ambient light sensor
	not support

	NFC
	no

	encryption card
	not support


Dimensions
	Length (mm)
	78

	Height (mm)
	53

	Thickness (mm)
	26

	Weight (g) Approx
	


Other Network Functions
	video intercom
	Support law enforcement instrument to platform single and two-way video intercom, support law enforcement instrument end-to-end single and two-way video intercom (requires integration of third-party software SDK)

	Voice cluster intercom
	Support group intercom, end-to-end intercom

	voice broadcast
	Support TTS voice broadcast

	voice control
	Currently, it can only support Chinese, and other languages need to integrate third-party speech algorithms or secondary development

	Facial and license plate recognition
	support

	network standard
	Global frequency band
4G:
TDD(38/39/40/41)
FDD(B1/2/3/4/5/7/8/20/28AB)
CDMA:BC0

	Platform Administration software
	Support real-time preview/real-time positioning/trajectory playback/intercom/monitoring/remote command issuance, etc.(support secondary development of API calls, independent platform deployment, or secondary independent development of independent key values)

	text overlay
	Support stacking time, equipment number, law enforcement officer number, location information, speed information, and support stacking in Chinese

	Command and dispatch platform docking
	Support protocols: Support platforms such as 808, GB/T28181, RTMP, RTSP, ONVIF protocols and other mainstream protocols in the market to connect with audio and video, intercom, and location device information.


Basic Device Functions
	Video extension
	support

	Video pre-recording
	support

	Impact alarm
	Support airbag security. The product needs to have a G sensor, which can record drops and record collisions. If it has a 4G function, it can be linked in the background.

	video encryption
	Supports AES256 encryption-SHA1-SHA2

	night vision
	Automatic or manual night vision switching, support for high-power red lights

	fill light
	Support the use of white LEDs for auxiliary lighting in dark situations.

	menu language
	Default Simplified Chinese/English (other languages can be customized)

	USB flash drive function
	Drive mode: After connecting to the computer, you can enter the USB flash drive mode (removable hard disk) through the upper computer on the PC side;
Non-drive mode: After connecting to the computer, directly enter USB flash drive mode (removable hard disk); one of the two modes can be selected

	continuous shooting function
	The supporting device can take more than 10 photos continuously at one time

	Key Document Marker
	You can mark this video file by pressing the corresponding button during the recording process;

	One-click shortcut function
	no

	password protection function
	support

	in-vehicle functions
	not support

	Shooting in the middle
	During the recording process, press the shoot button to take a photo individually

	acquisition station
	Support collection station and background management 1. Operation logs;2. Data collection and classification

	data security management
	Law enforcement recorders have different authority management. Primary authority can only view and playback law enforcement videos, photos, and recordings, and cannot delete or modify sensitive settings of the machine. Sensitive settings of the machine can only be made through password verification, and can only be copied, modified or deleted after connecting to a computer.

	automatically overwritten
	Support automatic override/non-override

	Close beat mode
	Support no indicator light display and no sound reminder mode.

	safe mode
	Safe mode is limited to basic operations such as recording, taking photos, and recording. A password is required to enter the settings interface and playback interface.


Others
	protection grade
	IP68 fell 2 meters

	injection molding process
	Two-color mold process (anti-crack)

	operating temperature
	-20~55℃

	low-temperature compatibility
	Corresponding low-temperature batteries should be prepared for inspection and low-temperature areas. The low-temperature-30 ℃ battery life of a single battery should be more than 2 hours. Normal temperature batteries should be standard. Normal temperature batteries and low-temperature batteries have different densities and operating environments.

	Storage relative humidity
	63%(30℃)

	storage temperature
	-40~60℃

	operating relative humidity
	40%~80%
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Universal Optional Accessories
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Polyester single shoulder strap
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Reflective shoulder straps
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Reflective shoulder strap




image13.jpg
WA

Shoulder straps on both shoulders




image14.jpg
BABBH Single shoulder strap




image15.jpg
HIal RE U (B R E

Wear law enforcement device accessories
leather case on the chest
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Law enforcement equipment accessorieslather cover
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Anti slip fixed headband bracket
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Car suction cup holder
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360 degree metal head long shoulder clip
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180 degree plastic head long shoulder clip
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Polyester shoulder strap




