K6-Semiconductor alcohol tester
Product Specification (Model: )
Product Information
	Appearance Name
	K6B

	Series Model
	

	Features
	High cost performance, high sensitivity in low temperature environments, and sensor with preheating function


Six Views
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Function Diagram
	[image: ]


Alcohol Test Basic Parameters
	Warning lamp shade color
	Available in red, blue or white

	Body color
	black

	product name
	Breath alcohol tester

	display screen
	1.44 Inch 128*128 full-color TFT LCD screen

	power supply
	18650-2000mAh lithium battery (built-in battery)

	charging voltage
	5V1A

	operating temperature
	-5℃~45℃

	Continuous measurement time
	5 seconds to 15 seconds

	value out time
	3 seconds

	Voice broadcast (language)
	Chinese/English

	sampling mode
	Blow sensing or manual detection

	using the sensor
	semiconductor gas sensor

	Measurement range of alcohol concentration in breath
	0~400mg/100mL

	accessibility
	LED highlight white light lighting, high-decibel whistle, red and blue warning lights, voice playback

	operation mode
	4 buttons to operate warning lights, police whistles and lights

	Sensitivity/Resolution
	5mg/100mL/    1mg/100mL

	Product size
	310*40.5*40.4mm

	product Weight
	Approximately 172g

	indication error
	±10mg/100 ml at a concentration of 50mg/100 ml at a distance of 5cm


Packing Information
	Box gauge: length × width × height mm
	38×28×36 CM

	Number of boxes:
	20 PCS/box

	Weight of the whole box:
	8.4KG   Gross weight 8.95KG

	Package: L × W × H mm
	340×85×50 MM

	Net weight of packaging box:
	248 g

	Machine net weight:
	175g

	Weight of outer packaging box:
	1/KG
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