WBO-Power replacement 1080P
Product Specification (Model: WBO-换电1080P)
Product Information
	Appearance Name
	WBO

	Series Model
	WBO-换电1080P


Six Views
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Function Diagram
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Basic Information
	processor
	no

	operating system
	no

	Screen size
	2.0 inch horizontal screen

	Default battery capacity
	1800mAh

	charging duration
	3 hours

	Continuous recording duration
	about 13 hours

	standby time
	empty

	anti-shake
	no

	image format
	AVI

	compression format
	MPEG

	Video size
	Max. 1080P (1920*1080)30FPS

	photo format
	JPEG

	horn
	1W

	body memory
	Scalable up to 512G

	Rear camera (main)
	100W

	Photo size
	Maximum 58 million


Lighting
	laser lamp
	no

	alarm lamp
	Red and blue warning lights

	infrared lamp
	have

	white light Lamp
	have


Interfaces
	charging interface
	Type-C

	G-sensor
	not support

	vibration motor
	not support

	external camera
	not support

	charging base
	support

	charging method
	Complete machine + battery compartment

	charger
	5V-1A

	USB interface
	USB 2.0


Data Functions
	WIFI
	no

	Bluetooth/433
	no

	positioning
	no


Dimensions
	Length (mm)
	

	Height (mm)
	

	Thickness (mm)
	

	Weight (g) Approx
	


Basic Device Functions
	Video extension
	support

	Video pre-recording
	not support

	Built-in small battery
	None-Change battery and power off

	Replace the battery without power
	When the device is in use, remove the main battery and continue to maintain normal recording status

	Impact alarm
	no

	video encryption
	not support

	night vision
	Automatic or manual night vision switching, support for high-power red lights

	fill light
	Support the use of white LEDs for auxiliary lighting in dark situations.

	menu language
	Default Simplified Chinese/English (other languages can be customized)

	USB flash drive function
	Drive mode: After connecting to the computer, you can enter the USB flash drive mode (removable hard disk) through the upper computer on the PC side;
Non-drive mode: After connecting to the computer, directly enter USB flash drive mode (removable hard disk); one of the two modes can be selected

	Key Document Marker
	You can mark this video file by pressing the corresponding button during the recording process;

	continuous shooting function
	The supporting device can take more than 10 photos continuously at one time

	password protection function
	support

	automatically overwritten
	Support automatic override/non-override

	Shooting in the middle
	During the recording process, press the shoot button to take a photo individually

	safe mode
	Safe mode is limited to basic operations such as recording, taking photos, and recording. A password is required to enter the settings interface and playback interface.

	Close beat mode
	Support no indicator light display and no sound reminder mode.

	in-vehicle functions
	Support vehicle-mounted certificate collection, and realize automatic video recording and evidence collection when the car ignites and turns on, and automatic shutdown after parking and flameout.

	acquisition station
	Support collection station and background management 1. Operation logs;2. Data collection and classification

	data security management
	Law enforcement recorders have different authority management. Primary authority can only view and playback law enforcement videos, photos, and recordings, and cannot delete or modify sensitive settings of the machine. Sensitive settings of the machine can only be made through password verification, and can only be copied, modified or deleted after connecting to a computer.

	One-click shortcut function
	Support one-click quick start of recording, one-click start of recording function (no need to start the power button separately)

	motion detection
	Supports automatic recording and stopping of recording based on scene changes and still


Others
	protection grade
	IP50 fell 2 meters

	injection molding process
	monochrome injection molding

	low-temperature compatibility
	Corresponding low-temperature batteries should be prepared for inspection and low-temperature areas. The low-temperature-30 ℃ battery life of a single battery should be more than 2 hours. Normal temperature batteries should be standard. Normal temperature batteries and low-temperature batteries have different densities and operating environments.

	Storage relative humidity
	63%(30℃)

	storage temperature
	-40~60℃

	operating relative humidity
	40%~80%

	operating temperature
	-20~55℃


Packing Information
	Box gauge: length × width × height mm
	

	Number of boxes:
	40 PCS/box

	Weight of the whole box:
	

	Package: L × W × H mm
	

	Net weight of packaging box:
	

	Machine net weight:
	

	Weight of outer packaging box:
	550g


Standard Accessories
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Dedicated Optional Accessories
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Universal Optional Accessories
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Magnetic Chest Clip
Magnetic Chest Clip
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Pin brooch clip
Pin brooch clip
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Polyester shoulder strap

Polyester shoulder strap




image13.jpg
Polyester single shoulder strap
Polyester single shoulder strap
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Reflective shoulder straps
Reflective shoulder straps
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Reflective shoulder strap
Reflective shoulder strap
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Double shoulder straps
shoulder straps on both shoulders
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Single shoulder strap Single shoulder strap
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Wear a law enforcement accessories holster on your chest

Wear law enforcement device accessories
leather case on the chest
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Leather case for law enforcement accessory

Law enforcement equipment accessories leather cover
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Anti-slip fixed headband bracket
Anti slip fixed headband bracket
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B1TZEX 2 bicycle stand
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TR MIFE Magnetic chest clip
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B3 Shoulder clip
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B#T3% Shoulder lamp clip
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A FF Walkie talkie clip
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28R Crocodile back clip
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Car suction cup holder
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fase Chest clip
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Long Clip LONG CLIP
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/&% Small back clip
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BB Plastic shoulder clip
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#l§tk  Pinclip
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kiR Large board clamp
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JB4T shoulder light
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360 degree metal head long shoulder clip
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180 degree plastic head long shoulder clip
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4@B¥K Shortshoulder clip
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B% Shoulder clip (2)
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B% Shoulder clip (1)
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Charger CHARGER PLUG
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quarter-inch adapter
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Data Cable USB CABLE
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Battery battery
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Charging case Charging case
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Tripod tripod
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Waterproof leather gloves
Waterproof leather case




