K1-Electrochemical alcohol tester
Product Specification (Model: )
Product Information
	Appearance Name
	K1

	Series Model
	

	Features
	High anti-interference and precision, high sensitivity


Six Views
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Function Diagram
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Alcohol Test Basic Parameters
	Warning lamp shade color
	Available in red, blue or white

	Body color
	black

	product name
	Fuel cell type exhaled gas alcohol tester

	display screen
	1.29-inch OLED color display

	power supply
	18650-3000mAh lithium battery

	charging voltage
	5V2A

	operating temperature
	-5℃~45℃

	Continuous measurement time
	1 to 15 seconds

	value out time
	3 seconds

	Voice broadcast (language)
	Chinese/English

	sampling mode
	Blow sensing or manual detection

	using the sensor
	fuel cell sensor

	Measurement range of alcohol concentration in breath
	0~200mg/100mL BAC

	accessibility
	LED highlight white light lighting, high-decibel whistle, red and blue warning lights, voice playback

	operation mode
	4 buttons, warning lights, alarm whistles and lights can be independently operated when shutdown is performed

	Sensitivity/Resolution
	5mg/100mL/    1mg/100mL

	Product size
	262mm*φ45mm

	product Weight
	Approximately 265g

	indication error
	no


Packing Information
	Box gauge: length × width × height mm
	42x29x30CM

	Number of boxes:
	20 PCS/box

	Weight of the whole box:
	10.2KG   Gross weight 10.8KG

	Package: L × W × H mm
	290*60*110 MM

	Net weight of packaging box:
	225g

	Machine net weight:
	265g

	Weight of outer packaging box:
	550g
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